From 6a05f26e4a7726fa719a55b5918b0262b27c02ba Mon Sep 17 00:00:00 2001
From: xengineering <me@xengineering.eu>
Date: Sun, 14 Jan 2024 20:48:43 +0100
Subject: doc: Simplify streaming commands

---
 doc/documentation.tex | 8 ++++----
 1 file changed, 4 insertions(+), 4 deletions(-)

(limited to 'doc/documentation.tex')

diff --git a/doc/documentation.tex b/doc/documentation.tex
index a74403d..230f25c 100644
--- a/doc/documentation.tex
+++ b/doc/documentation.tex
@@ -72,16 +72,16 @@ As soon as the soundbox is listening the stream can be send from another
 computer in the same network with this command:
 
 \begin{verbatim}
-	ffmpeg -re -f lavfi -i aevalsrc="sin(400*2*PI*t)" -ar 8000 -f mulaw \
-	    -f matroska udp://224.0.0.99:5316
+	ffmpeg -re -f lavfi -i aevalsrc="sin(400*2*PI*t)" \
+	    -acodec libmp3lame -f matroska udp://224.0.0.99:5316
 \end{verbatim}
 
 It will send a simple sine wave with 400~Hz to the soundbox device.
 Alternatively a MP3 file can be sent like this:
 
 \begin{verbatim}
-	ffmpeg -re -i <file-path> -acodec copy -ar 11025 \
-	    -f matroska udp://224.0.0.99:5316
+	ffmpeg -re -i <file-path> \
+	    -acodec copy -f matroska udp://224.0.0.99:5316
 \end{verbatim}
 
 These commands allow to test the \texttt{soundbox} device setup.
-- 
cgit v1.3

