From cad96e8944a86df30376564dca15661ddef590a4 Mon Sep 17 00:00:00 2001
From: xengineering <me@xengineering.eu>
Date: Fri, 5 Jan 2024 20:58:34 +0100
Subject: doc: Switch from UDP port 1234 to UDP port 5316

This port should be used in the future as soundbox standard port.
---
 doc/documentation.tex | 8 ++++----
 1 file changed, 4 insertions(+), 4 deletions(-)

(limited to 'doc/documentation.tex')

diff --git a/doc/documentation.tex b/doc/documentation.tex
index eea482a..967b89d 100644
--- a/doc/documentation.tex
+++ b/doc/documentation.tex
@@ -61,10 +61,10 @@ For a simple audio streaming test the following commands from the FFmpeg
 streaming
 guide\footnote{\href{https://trac.ffmpeg.org/wiki/StreamingGuide\#StreamingasimpleRTPaudiostreamfromFFmpeg}{https://trac.ffmpeg.org/wiki/StreamingGuide\#StreamingasimpleRTPaudiostreamfromFFmpeg}}
 can be used. The following command has to be executed on the soundbox to start
-listening on port \texttt{1234} for incoming audio streams:
+listening on port \texttt{5316} for incoming audio streams:
 
 \begin{verbatim}
-	ffplay rtp://127.0.0.1:1234
+	ffplay rtp://127.0.0.1:5316
 \end{verbatim}
 
 As soon as the soundbox is listening the stream can be send from another
@@ -72,7 +72,7 @@ computer in the same network with this command:
 
 \begin{verbatim}
 	ffmpeg -re -f lavfi -i aevalsrc="sin(400*2*PI*t)" -ar 8000 -f mulaw \
-	    -f rtp rtp://<soundbox-ip>:1234
+	    -f rtp rtp://<soundbox-ip>:5316
 \end{verbatim}
 
 It will send a simple sine wave with 400~Hz to the soundbox device.
@@ -80,7 +80,7 @@ Alternatively a mp3 file can be sent like this:
 
 \begin{verbatim}
 	ffmpeg -i '/path/to/file.mp3' -acodec libmp3lame -ar 11025 \
-	    -f rtp rtp://<soundbox-ip>:1234
+	    -f rtp rtp://<soundbox-ip>:5316
 \end{verbatim}
 
 These commands allow to test the \texttt{soundbox} device setup.
-- 
cgit v1.2.3-70-g09d2

