From e7f055deddf551c32de631c4579c53589ea14948 Mon Sep 17 00:00:00 2001
From: xengineering <me@xengineering.eu>
Date: Sat, 20 Jan 2024 15:12:42 +0100
Subject: doc: Split configuration section into subsections

---
 doc/documentation.tex | 8 ++++++++
 1 file changed, 8 insertions(+)

(limited to 'doc/documentation.tex')

diff --git a/doc/documentation.tex b/doc/documentation.tex
index ba9aab3..fb004f7 100644
--- a/doc/documentation.tex
+++ b/doc/documentation.tex
@@ -183,6 +183,8 @@ With this setup the Alpine Linux installation is completed.
 
 \section{Configure Alpine Linux for soundbox}
 
+\subsection{Package installation}
+
 soundbox requires packages from the Alpine Linux community package repository.
 Since this is not enabled by default it has to be done manually. This can be
 done by editing the \texttt{/etc/apk/repositories} file with an editor like
@@ -219,6 +221,8 @@ wpa_supplicant' > /etc/apk/world
 apk add
 \end{verbatim}
 
+\subsection{LLDP network discovery}
+
 To make the soundbox device discoverable inside the network the Link Layer
 Discovery Protocol (LLDP) is used. With \texttt{echo} a new configuration file
 for the \texttt{lldpd} software can be added. After configuration the
@@ -232,6 +236,8 @@ configure lldp agent-type nearest-customer-bridge' \
 rc-update add lldpd default
 \end{verbatim}
 
+\subsection{Audio configuration}
+
 The only user on a soundbox device is \texttt{root}. Even that super user has
 to be added to the \texttt{audio} group to be able to play sound via ALSA. This
 can be achieved with \texttt{addgroup}.
@@ -258,6 +264,8 @@ option has to be inserted instead:
 echo 'dtparam=audio=on' >> /media/mmcblk0p1/config.txt
 \end{verbatim}
 
+\subsection{Persistence of changes and reboot}
+
 Since a diskless Alpine Linux installation is preferred for soundbox the
 changes have to be made persistent with \texttt{lbu}. Rebooting after it makes
 sure the SD card is again mounted in read-only mode and all Kernel-affecting
-- 
cgit v1.2.3-70-g09d2

